Mish {#dev_guide_op_mish}
=========================

## General

Mish performs element-wise activation function on a given input tensor, based 
on the following mathematical formula:
\f[ dst = src * \tanh(SoftPlus(src)) = src * \tanh(\ln(1 + e^{src})) \f]

## Operation attributes

Mish operation does not support any attribute.

## Execution arguments

The inputs and outputs must be provided according to below index order when
constructing an operation.

### Inputs

| Index | Argument Name | Required or Optional |
|:------|:--------------|:---------------------|
| 0     | `src`         | Required             |

### Outputs

| Index | Argument Name | Required or Optional |
|:------|:--------------|:---------------------|
| 0     | `dst`         | Required             |

## Supported data types

Mish operation supports the following data type combinations.

| Src  | Dst  |
|:-----|:-----|
| f32  | f32  |
| bf16 | bf16 |
| f16  | f16  |
